

(A)

(B)

Figure SI 3: Variation of the peak current with MP concentration in 0.1 M PBS (pH 6.67) on GCE/NiAl-BEHP, from 0.5 µM to 12 µM. The inset shows the corresponding calibration of nitro (A) and (B) nitroso groups